THE REQD RANGE IS 120W-140W ,EVEN THOUGH WE HAVE MENTIONED YOU MAY DECIDE THE WATTAGE AS PER SPEC ENCLOSED FOR COMPLIANCE POINT BY POINT ,PLS FILL UP THE SAME WITH YOUR REMARKS & THE REPORT/DOCUMENTS AS REQD SHALL BE SENT