**Additional Specifications Required**

1)      Additional Surge 10KW & 10 KA. With separate surge arrester of 440 Volt compliance.

2)      Wattage 120W with negative tolerance.

3)      Efficacy 130LM/W of full way light fitting. Not LED.

4)      Integrated Lens.

5)      440 Volt Compliance Phase to Phase.