

Halonix/Delhi/SML/2019-20/01 Date: - 28th July 2019

**To,**

**WATER POWER ENGG. ENTERPRISES**

**Regd. Office: M-37A, IInd Floor,**

**Rajouri Garden, New Delhi-110027**

**Kind Attn: - Mr. Rajesh Arora**

**SUBJECT: Offer for Halonix make LED Lights against your Inquiry.**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Sr. No** | **Item Description** | **Item Code** | **photo** | **Qty** | **Unit Price** | **GST** | **Net Amount** | **Total Value** |
| NS-13 | Supply and erection of 70-72W LED Street light fitting operating voltage single phase 230 volts AC, 50Hz conforming to CEE/NR Specification. No. CEE/NR/121- Elect./PS/2017 (Rev.-3) dated 28.06.2018 complete with all accessories, including connection with 2x2.5 sq.mm PVC insulated multi stranded FRLS copper conductor cable, testing, commissioning &earthing required and as per explanatory note. |  |  |  |  |  |  |  |
| NS-14 | Supply and erection of 18-20W LED tube light fitting 1200mm, T8, Indoor Type, System Efficacy 100 lm/W (+/- 5%), conforming to CEE/NR Specification. No. CEE/NR/121-Elect./PS/2017(Rev.-3) dated 28.06.2018 complete with all accessories, including connection with 2x2.5 sq.mm PVC insulated multi stranded FRLS copper conductor cable, testing, commissioning &earthing required and as per explanatory note |  |  |  |  |  |  |  |
| NS-15 | Supply, testing and fixing of 08-10 Watts LED Bolard light fitting conforming to CEE/NR Specification. No. CEE/NR/121-Elect./PS/2017 (Rev.-3) dated 28.06.2018 complete with all accessories, connections with 2x2.5 sq.mm PVC insulated multi stranded FRLS copper conductor cable testing, commissioning &earthing required and as per explanatory. |  |  |  |  |  |  |  |
| NS-16 | Supply and erection of 10 Watts Bulk Head LED fitting conforming to CEE/NR Specification. No. CEE/NR/121- Elect./PS/2017 (Rev.-3) dated 28.06.2018 complete with all accessories, connection with 2x2.5 sq.mm PVC insulated multi stranded FRLS copper conductor cable testing, commissioning &earthing required and as per explanatory |  |  |  |  |  |  |  |
| NS-18 | Supply, testing and fixing of 9/10 Watts LED bracket light fitting conforming to CEE/NR Specification. No. CEE/NR/121-Elect./PS/2017 (Rev.-3) dated 28.06.2018 complete with all accessories, connections with 2x2.5 sq.mm PVC insulated multi stranded FRLS copper conductor cable testing, commissioning &earthing required and as per explanatory |  |  |  |  |  |  |  |
| NS-19 | Supply, testing and fixing of 7/9 Watts LED mirror light fitting conforming to CEE/NR Specification. No. CEE/NR/121-Elect./PS/2017 (Rev.-3) dated 28.06.2018 complete with all accessories, connections with 2x2.5 sq.mm PVC insulated multi stranded FRLS copper conductor cable testing, commissioning &earthing required and as per explanatory |  |  |  |  |  |  |  |
| NS-20 | Supply, testing and fixing of 18 Watts LED down lighter fitting Square/Round (Recess/Surface) complete with allaccessories including connections with 2x2.5 sq.mm PVC insulated multi stranded copper conductor cable including testing, commissioning &earthingrequiredasperCEE/NRSpecification. No. CEE/NR/121-Elect./PS/2017 (Rev.-3) dated 28.06.2018 and as per explanatory note. |  |  |  |  |  |  |  |

