

Halonix/Delhi/SML/2019-20/01 Date: - 28th July 2019

**To,**

**WATER POWER ENGG. ENTERPRISES**

**Regd. Office: M-37A, IInd Floor,**

**Rajouri Garden, New Delhi-110027**

**SUBJECT: Offer for Halonix make LED Lights against your Inquiry.**

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **S.No.** | **Item Code** | **Item Qty** | **Qty Unit** | **Unit Rate** | **GST extra** |  |  | **Item Code** | **Photo** |
| **Schedule** B-NON SCHEDULE ITEMS | | | | |  |  |  |  |  |
| 1 | NS-1 | 80 |  |  |  |  |  |  |  |
| **Item Description:-** Supply installation, testing & commissioning of 90W LED Street Light Fitting complete with all accessories as per explanatory note on erected pole including supply &wiring with 2x2.5 sq. mm PVC insulated multi-stranded ISI marked copper conductor cable from Jn. Box to fitting as per CEE/NR specification no.119-Elect/PS/2016 (Rev.01) | | | | | | | | |
| 2 | NS-2 | 290 | Numbers |  |  |  |  |  |  |
| **Item Description:-** Supply installation, testing & commissioning of of 45W LED Street Light Fitting complete with all accessories as per explanatory note on erected pole including supply &wiring with 2x2.5 sq. mm PVC insulated multi-stranded ISI marked copper conductor cable from Jn. Box to fitting as per CEE/NR specification no.119-Elect/PS/2016 (Rev.01) | | | | | | | | |
| 3 | NS-3 | 30 | Numbers |  |  |  |  |  |  |
| **Item Description:-** Supply, testing and fixing of 10 Watts Bulk Head LED fitting as per explanatory note including supply & wiring with 2x1.5 sq. mm PVC insulated multi-stranded ISI marked copper conductor cable from Jn. Box to fitting. | | | | | | | | |
| 4 | NS-4 | 330 | Numbers |  |  |  |  |  |  |
| **Item Description:-** Supply, testing and fixing of 7W LED bulb with built-in LED driver housed with BC base and as per CEE/NR specification no.119- Elect/PS/2016 (Rev.01) | | | | | | | | |
| 7 | NS-9A | 365 | Numbers |  |  |  |  |  |  |
| **Item Description:-** Supply and erection of 1X18W surface type LED tube light fittings complete with control panel & all accessories including connections with 2x2.5 sq.mm PVC insulated multi stranded copper conductor cable including testing, commissioning &earthing required as per Specification. No. 118-Elect./PS/2014 and as per explanatory note. | | | | | | | | |
| 8 | NS-9B | 310 | Numbers |  |  |  |  |  |  |
| **Item Description:-** Supply and erection of 2X18W surface type LED tube light fittings complete with control panel & all accessories including connections with 2x2.5 sq.mm PVC insulated multi stranded copper conductor cable including testing, commissioning &earthing required as per Specification. No. 118-Elect./PS/2014 and as per explanatory note. | | | | | | | | |
| 12 | NS-25 | 27 | Numbers |  |  |  |  |  |  |
| **Item Description:-** Supply of Less than or equal to 150W (More than or equal to 16000 Lumen) LED Light Fitting complete with all accessories as per explanatory note to be fixed on High Mast including testing, commissioning and earthing including supply & wiring with 2x2.5 sq. mm PVC insulated multi-stranded ISI marked copper conductor cable from Jn. Box to fitting as per CEE/NR specification no.119-Elect/PS/2016 (Rev.01) | | | | | | | | |